SERVO CONFIGURATION

Pin 0 right eye — pupil horizontal

Pin 1 right eye — pupil vertical

Pin 2 right eye — eyelid closure

Pin 3

Pin 4 right eyebrow

Pin 5 mouth — right rotation

Pin 6

Pin 7

Pin 8

Pin 9

Pin 10 mouth — left rotation

Pin 11 left eyebrow

Pin 12

Pin 13 left eye — eyelid closure

Pin 14 left eye — pupil vertical

Pin 15 left eye — pupil horizontal

*(The servo’s yellow wire should be on top, the brown wire should be on the bottom)*

